Search Port Cnt = 2!
Please reset the STB!
BOOTROM ...
03:16:22--Start Calibration ...
03:16:22--CLOCK_OFFSET = -17 
DELAY_90_OFFSET = 0 
DELAY_9090_OFFSET = 0 
DQS_IN_90_OFFSET = 0 
03:16:22--0:range 2 start = 0  end = 0 rl_add_i = 4
03:16:22--0:range 2 start = 0  end = 1 rl_add_i = 4
03:16:22--0:range 2 start = 0  end = 2 rl_add_i = 4
03:16:23--0:range 2 start = 0  end = 3 rl_add_i = 4
03:16:24--0:range 2 start = 14  end = 14 rl_add_i = 4
03:16:24--0:range 2 start = 14  end = 15 rl_add_i = 4
03:16:24--0:range 2 start = 14  end = 16 rl_add_i = 4
03:16:24--0:range 2 start = 14  end = 17 rl_add_i = 4
03:16:24--0:range 2 start = 14  end = 18 rl_add_i = 4
03:16:24--0:range 2 start = 14  end = 19 rl_add_i = 4
03:16:25--0:range 2 start = 14  end = 20 rl_add_i = 4
03:16:25--0:range 2 start = 14  end = 21 rl_add_i = 4
03:16:25--0:range 2 start = 14  end = 22 rl_add_i = 4
03:16:25--0:range 2 start = 14  end = 23 rl_add_i = 4
03:16:25--0:range 2 start = 14  end = 24 rl_add_i = 4
03:16:25--0:range 2 start = 14  end = 25 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 26 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 27 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 28 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 29 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 30 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 31 rl_add_i = 4
03:16:26--0:range 2 start = 14  end = 32 rl_add_i = 4
03:16:27--0:range 2 start = 14  end = 33 rl_add_i = 4
03:16:27--0:range 2 start = 14  end = 34 rl_add_i = 4
03:16:27--0:range 2 start = 14  end = 35 rl_add_i = 4
03:16:27--0:range 2 start = 14  end = 36 rl_add_i = 4
03:16:27--0:range 2 start = 14  end = 37 rl_add_i = 4
03:16:28--rang0: 00 0 0 , rang1: 00 0 0 , rang2: 24 1 0, rang3: 00 0 0 
03:16:28--DDR2 Calibiration param is: clk star 14, end 37, rdclk_rising_latch 1, digclk_neglatch 0, rd_add 4 
03:16:28--0xa4 = 33339000
03:16:28--0x38 = 72140001
03:16:28--0x50 = 00190910
03:16:28--0x4c = 000a1001
03:16:28--0x44 = 001d0000
03:16:28--0x54 = 0a0a0a0a
03:16:28--Calibration done, cost 5 s
DDR Calibration SUCCESS
Got sync byte!
Start sending client...
Start to check serial...

Prepare to download...

Start downloading data...

End downloading

Verify burning flash...
Start burning flash, DONOT POWOFF!

Burning flash OK!

OST¹Am

U-Boot 2012.04 (Aug 19 2014 - 15:13:05)

Board: mips CPU: 4KWDRAM:  128 MiB
flash_init: size=0x800000, sec cnt=2048, ID= 0x170000
Flash: 8 MiB
*** Warning - bad CRC, using default environment

In:    serial
Out:   serial
Err:   serial
Net:   ^^^^^^^^^^^^^^^^ethernet reset 58****************
mt_eth
main_loop entered: bootdelay=0

Hit any key to stop autoboot:  0 
uboot_auto FastLogo_TaskStart
boot_jump_ID=0x89,back_addr=0xb0002000,boot_para1=0xbfef0188, data=10x12345678
boot_para2=0xbfef018c, data2=0x0
boot_para3=0xbfef0190, data3=0x89364421

 1. mem_start[800cb008]

 2. system memory size[8000000]
SYS_PARTITION_SIZE is 1e00000, EPG_BUFFER_ADDR is 6d7d000
create SYS_PARTITION1 ok!
init mem11 ok!
Enable irq!
mem_cfg
drv_init
set header 0xC
set header dm hdr start addr
i2c attach
uio attach
uio init end
display attach
load_logo,line = 698:app_blk_num=16
load_logo,line = 719:block_size=376632,block_id=93
start_logo_ticks=27,addr=0xa6e94000
end_logo_ticks=52
goto ota
boot_para3=bfef0190,*boot_para3=12340001
FastLogo_TaskEnd
m

U-Boot 2012.04 (Aug 19 2014 - 15:13:05)

Board: mips CPU: 4KWDRAM:  128 MiB
flash_init: size=0x800000, sec cnt=2048, ID= 0x170000
Flash: 8 MiB
*** Warning - bad CRC, using default environment

In:    serial
Out:   serial
Err:   serial
Net:   ^^^^^^^^^^^^^^^^ethernet reset 58****************
mt_eth
main_loop entered: bootdelay=0

boot is reback from APP!

MaincodeTaskStart

 Built at Nov 27 2014--11:37:09 

 1. mem_start[80dab178]

 2. system memory size[8000000]
SYS_PARTITION_SIZE is 1500000, GUI_RESOURCE_BUFFER_ADDR is 244d000
free mem 1711752
Os version pass!
Enable irq!
xxxxxxxxxxxxxxxxx




zzzzzyyyyyyyyyyyyyyyyyyy




mem_cfg
util_init
block attach 1
*******usb1****
*****block(USB/SD) attached && open******

 
charto attach
dm init v2
dma init
set header [0xC]
set header [0x60000]

**** SYSTEM_MEMORY_END[0x834d6000]***
file_size 2466341 p_data_buffer 80e4f430 

 unzip resource. in_addr = 0x9041e11c, out_addr = 0x8244d000, in_len = 2466341, out_len = 12815144
i2c attach
uio attach
uio init end
nim attach
tuner 1 open addr 0x80dffbb0
*********hdmi config value=12340001
*********hdmi is config
display attach
gpe vsb attach
dmx attach
audio vsb attach
vdec attach
drv_init hour1=0,minute1=0
pdec attach
tcpip: Oct 31 2014 11:15:04/nthread task for ethernet 10 
attach wifi
set_wifi_device_status 0
set_wifi_device_status-2 0
rtl8188eus_ethernet_attach p_dev80e25c70 p_wifi_dev 80e25d50 p_lld 80e25cc0 p_lld_addr 80e25c74 
attach wifi success
attach wifi
<===mtk_mt5370u_series_attach,usb_wifi_ralink

 #########task info########### 
g_Mtk_task_let_0[13]MTK_WIFI_TASK_TIMERQ[14]
MTK_WIFI_TASK_MlmeThread[8]MTK_WIFI_TASK_RTUSBCmdThread[9]
g_wifi_wpa_supplicant_task_prio_ra0 16

 #########task info  done ########### 
attach wifi success
lcp_init: xmit_accm=0 0 0 0
upap_init: 0
serial_open
Set flash Status REG=[0x0]
set mid[c8] protect status[0] type[0]Success
driver init time = 5670 ms
drv_init
dm set cache
dm set cache is done
g_status size 7200


*********************long_str_store.end_pos 2611


----------------------------------------
 Software version is 1162
----------------------------------------

mdl init time = 90 ms
mid_init
app_init
ui init time = 0 ms
ui_init
------
¿¿ÿÿ¿µÿü¿½½ÿî\½¿ÿX½­ÿ(é½Õýÿï¿ÿ¿¿ÿÿÿ¼ü°½½½½­­­í½½¿½½ÿ¾½½¿½½½½½½½¼½½½½­­­­­½½½½½½½½½¼½½½½­­­­­­­+©­­ý½¹©©©©©ý½½½½½½½½½½½­­­­­­-©¥­ý½½½½½½½½½¼½½­½½